

**Industrial Panel PC**

**QY-P5320**

**Products Features:**

1. **Industrial-Grade Embedded Fanless Panel PC**
2. **32 inch LED Screen, Resolution: 1920\*1080**
3. **Support Capacitive Touch Screen**
4. **Intel Celeron and Core 4/7/8/10/11/12/13th-i3/i5/i7 CPU**
5. **2\*RJ-45, 4\*USB, 2\*COM, 1\*HDMI, 1\*VGA**
6. **Support 4G/5G and WIFI module**
7. **DC 12V Power Input**
8. **-20℃~50℃ Temperature Can Keep 24/7 Work Stably**
9. **Front Panel IP65 Water proof**

**QY-P5320**

**1.Mother Board Specification:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **QY-P5320** | | |
| **CPU** | **J1900**  **i3-4010U**  **i5-4260U**  **i7-4650U** | **J6412**  **i3-7100U / 8130U / 10110U**  **i5-7200U / 8250U / 10310U**  **i7-7500U / 8550U / 10710U** | **N95 / N100**  **i3-1115G4 / 1215U / 1315U**  **i5-1135G7 / 1235U / 1335U**  **i7-1195G7 / 1255U / 1270P / 1355U** |
| **Memory[1]** | **2\*DDR III RAM Slots**  **Up to 16GB** | **2\*DDR IIII RAM Slots**  **Up to 32GB** | **2\*DDR IIII RAM Slots**  **Up to 64GB** |
| **Storage** | **1\*MSATA SSD Slot** | **1\*M.2 NVME SSD Slot** | |
| **1\*SATA SSD Slot** | | |
| **Display[2]** | **1\*HDMI: Resolution up to 4096\*2106@60Hz**  **1\*VGA: Resolution up to 1920\*1200@60Hz** | | |
| **Expansion** | **2\*Mini PCIE Slots**  **Support 4G and WIFI module** | **1\*M.2 and 1\*Mini PCIE Slots**  **Support 4G/5G and WIFI module** | **2\*M.2 Slots**  **Support 4G/5G and WIFI module** |
| **Ethernet** | **2\*RTL8211F LAN Chip (10 / 100 / 1000 Mbps, RJ-45 Type)** | | |
| **USB** | **4\*USB 3.0 (Type-A)** | | |
| **COM** | **1\*RS-232+1\*RS-485 / 232 (DB9 Type)**  **Support optional 6\*COM ports (Phoenix Terminal Type)** | | |
| **Audio** | **1\*MIC+1\*SPK** | | |

**Notes:**

**[1]: The maximum memory capacity and the maximum capacity per strip supported by this motherboard depend on the CPU.**

**[2]: The maximum resolution and frame rate of the display interface output depends on the CPU.**

**If you need other specifications, please refer to [P5000 Series Optional Specifications List].**

**QY-P5320**

**2.Screen Specification:**

|  |  |
| --- | --- |
| **Screen Size** | **32 inch TFT LED Screen, 16:9 Size** |
| **Resolution** | **1920\*1080** |
| **Brightness** | **350nits** |
| **Contrast** | **800:1** |
| **Largest Colorful** | **16M** |
| **Touch Screen Type** | **Capacitive** |
| **Transmittance** | **More than 95%** |
| **Touch Life** | **50 million times** |
| **Response Time** | **＜5ms** |
| **Touch Hardness** | **6 Mohs** |
| **Protection** | **Front Panel IP65 Water Proof** |

**QY-P5320**

**3.Device Specification:**

|  |  |
| --- | --- |
| **Power Input** | **DC 12V**  **(Support Optional DC 9-36V Wide Voltage Power Module)** |
| **Support Auto-Start** |
| **1\*2.5mm circle type DC Plug** |
| **Structure** | **Fully Enclosed Aluminum Alloy Material** |
| **Heat Dissipation** | **Fanless Design, Conduction Heat Dissipation** |
| **Installation** | **Desktop / Wall Mount** |
| **Size** | **749.2mm\*446.7mm\*64.8mm** |
| **System** | **Windows and Linux** |

**QY-P5320**

**4.Ordering Information:**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model** | **CPU** | **LAN** | **USB** | **COM** | **RAM** | **SSD** | **Expansion** | **Power** |
| **P5320** | **J1900** | **2** | **4** | **1\*RS-232/485**  **1\*RS-232** | **1\*DDR 3**  **Up to 8GB** | **1\*MSATA**  **1\*SATA** | **1\*Mini PCIE** | **DC 12V** |
| **4th** | **2\*DDR 3**  **Up to 16GB** | **2\*Mini PCIE** |
| **J6412** | **2\*DDR 4**  **Up to 32GB** |
| **7th / 8th** | **2\*DDR 4**  **Up to 32GB** | **1\*M.2 NVME**  **1\*SATA** | **1\*Mini PCIE**  **1\*M.2** |
| **10th** | **2\*DDR 4**  **Up to 64GB** |
| **N95 / N100** | **1\*DDR 4**  **Up to 16GB** | **2\*M.2** |
| **11th / 12th / 13th** | **2\*DDR 4**  **Up to 64GB** |

**5.Package List:**

|  |  |
| --- | --- |
| **Adapter** | **1\*12V 7A Adapter** |
| **Power Cable** | **1\*Power Cable** |

**QY-P5320**

**6.CPU Information:**

|  |  |  |
| --- | --- | --- |
| **CPU** | **Specification** | |
| **J1900** | **4 core, 4 total threads, 2.00 GHz to 2.40GHz, 2 MB cache** | **Max to 8GB for 1\*DDR 3 Slot** |
| **i3-4010U** | **2 core, 4 total threads, 1.70 Ghz, 3 MB Cache** | **Max to 16GB for 2\*DDR 3 Slots** |
| **i5-4260U** | **2 core, 4 total threads, 1.40 GHz to 2.70GHz, 3 MB cache** | **Max to 16GB for 2\*DDR 3 Slots** |
| **i7-4650U** | **2 core, 4 total threads, 1.70 GHz to 3.30GHz, 4 MB cache** | **Max to 16GB for 2\*DDR 3 Slots** |
| **N95** | **4 core, 4 total threads, 3.40GHz, 6 MB cache** | **Max to 16GB for 1\*DDR 4 Slot** |
| **N100** | **4 core, 4 total threads, 3.40GHz, 6 MB cache** | **Max to 16GB for 1\*DDR 4 Slot** |
| **J6412** | **4 core, 4 total threads, 2.00 GHz to 2.60GHz, 1.5 MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i3-7100U** | **2 core, 4 total threads, 2.40 GHz, 3MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i5-7200U** | **2 core, 4 total threads, 2.50 GHz to 3.10GHz, 3 MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i7-7500U** | **2 core, 4 total threads, 2.70 GHz to 3.50GHz, 4 MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i3-8130U** | **2 core, 4 total threads, 2.20 GHz to 3.40 GHz, 4MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i5-8250U** | **4 core, 8 total threads, 1.60 GHz to 3.40 GHz, 6MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i7-8550U** | **4 core, 8 total threads, 1.80 GHz to 4.00 GHz, 6MB cache** | **Max to 32GB for 2\*DDR 4 Slots** |
| **i3-10110U** | **2 core, 4 total threads, 2.10 GHz to 4.10 GHz, 4MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i5-10310U** | **4 core, 8 total threads, 1.70 GHz to 4.40 GHz, 6 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i7-10710U** | **6 core, 12 total threads, 1.10 GHz to 4.70 GHz, 12 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i3-1115G4** | **2 core, 4 total threads, 4.10 GHz, 6MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i5-1135G7** | **4 core, 8 total threads, 2.40 GHz to 4.20 GHz, 8MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i7-1165G7** | **4 core, 8 total threads, 2.80 GHz to 4.70 GHz, 12MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i3-1215U** | **6 core, 8 total threads, 40 GHz, 10MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i5-1235U** | **10 core, 12 total threads, 3.20 GHz to 4.40 GHz, 12MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i7-1255U** | **10 core, 12 total threads, 3.50 GHz to 4.70 GHz, 12MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i7-1270P** | **12 core, 16 total threads, 3.50 GHz to 4.80 GHz, 18 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i3-1315U (Coming soon)** | **6 core, 8 total threads, 3.30 GHz to 4.50 GHz, 10 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i5-1335U (Coming soon)** | **10 core, 12 total threads, 3.40 GHz to 4.60 GHz, 12 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |
| **i7-1355U (Coming soon)** | **10 core, 12 total threads, 3.70 GHz to 5.00 GHz, 12 MB cache** | **Max to 64GB for 2\*DDR 4 Slots** |

**7.System Information:**


|  |  |
| --- | --- |
| **CPU** | **System** |
| **J1900** | **Windows 7 / 10 and Linux** |
| **4th / 7th** |
| **N95 / N100 / J6412** | **Windows 10 / 11 and Linux** |
| **8th / 10th / 11th / 12th / 13th** |

**8.Fittings Information:**

**QY-P5320**

|  |  |  |
| --- | --- | --- |
| **RAM** | **DDR 3** | **4GB / 8GB** |
| **DDR 4** | **4GB / 8GB / 16GB / 32GB** |
| **SSD** | **MSATA** | **64GB / 128GB / 256GB / 512GB / 1TB** |
| **M.2 NVME** | **128GB / 256GB / 512GB / 1TB / 2TB / 4TB** |
| **SATA** | **120GB / 128GB / 240GB / 256GB / 480GB / 512GB / 960GB / 1TB / 2TB / 4TB** |
| **GSM Module** | **4G** | **4G+GPS** |
| **5G** | **5G+GPS** |
| **WIFI Module** | **7260AC / AX210** | |
| **Wide Voltage Power Module** | **DC 9-36V** | |

**QY-P5320**



**9.Dimensions:**