U Series Industrial Computer
QY-U1000



[image: 1U]





Products Features:
1. Industrial-Grade Embedded 1U Size Industrial Computer
2. Support Mini-ITX Mother Board
3. [bookmark: _GoBack]Intel 4/6/7/8/9/10/12/13/14th-i3/i5/i7/i9 Desktop CPU
4. Standard 1U ATX power, 300w to 1300w
5. More expansion slots, Mini PCIE / M.2 / PCIE
6. Support remote power on and off
7. -30℃~70℃ Temperature Can Keep 24/7 Work Stably
[image: 8223d1f8a58670e4cc7e820b3b72a5aa][image: 数据表背景图]
8. Anti-Static, Anti-Pulse, Anti-Surge, Anti-Radiation
Your Partner for Industrial Solutions
www.amodeipc.com
www.amodeipc.com
Your Partner for Industrial Solutions

QY-U1000
1-1.B81 Mother Board Specification:

	Mother Board Model
	QY-B81AH-H

	Chipset
	Intel B81, Support Intel Core 4th-i3/i5/i7 / Pentium / Celeron Desktop CPU, LGA 1150

	Memory
	Support DDR3-1333/1600 MHz, 2*non-ECC U-DIMM Slots, Up to 16GB

	Storage
	1*MSATA SSD slot
1*SATA 3.0 SSD slot
1*SATA 2.0 SSD slot

	Display
	1*HDMI: Resolution max up to 3840*2160@30hz
1*VGA: Resolution max up to 1920*1200@60Hz

	Expansion
	1*PCIE 16x slot
1*Mini PCIE slot, support 4G and WIFI module

	Ethernet
	2*Realtek 1Gbps LAN Chip (10 / 100 / 1000 Mbps, RJ-45 Type)

	USB
	6*USB 3.0 (Type-A)
10*USB 2.0 (Header)

	COM
	2*RS-232 (DB9 Type)
1*RS-232 / 485 (Box)
3*RS-232 (Box)
4*RS-232 (Header)

	Audio
	1*Line-out+1*Line-in+MIC

	Mother Board Type
	Mini-ITX





QY-U1000
1-2.H110 Mother Board Specification:

	Mother Board Model
	QY-B11AH-A

	Chipset
	Intel H110, Support Intel Core 6/7/8/9th-i3/i5/i7 / Pentium / Celeron desktop CPU, LGA 1151

	Memory
	Support DDR4-1866/2133 MHz, 2*non-ECC U-DIMM Slots, Up to 32GB

	Storage
	1*MSATA SSD slot
2*SATA3.0 SSD slots

	Display
	1*HDMI: Resolution max up to 4096*2160@24Hz
1*VGA: Resolution max up to 1920*1200@60Hz

	Expansion
	1*PCIE 16x slot
1*Mini PCIE slot, support 4G and WIFI module

	Ethernet
	2*Realtek GbE LAN Chip (10 / 100 / 1000 Mbps, RJ-45 Type)

	USB
	8*USB 3.0 (Type-A)
2*USB 2.0 (Type-A)
6*USB 2.0 (Header)

	COM
	2*RS-232 (DB9 Type)
1*RS-232 / 485 (Header)
7*RS-232 (Header)

	Audio
	1*Line-out+1*MIC

	Mother Board Type
	Mini-ITX






	
	Mother Board Model
	QY-H472A-X

	Chipset
	Intel H470 Support Intel Core 10th-i3/i5/i7/i9 / Pentium / Celeron desktop CPU, LGA 1200

	Memory
	Support DDR4-2133/2400/2666/2933 MHz, 2*U-DIMM Slots, Up to 64GB

	Storage
	1*M.2 SATA SSD slot
1*SATA3.0 SSD slot

	Display
	1*VGA: Resolution max up to 1920*1200@60Hz
1*HDMI: Resolution max up to 4096*2160@30Hz

	Expansion
	1*PCIE 16x slot
1*M.2 Key-E slot, support WIFI module

	Ethernet
	2*Realtek GbE LAN Chip (10 / 100 / 1000 Mbps, RJ-45 Type)

	USB
	6*USB 3.0 (Type-A)
4*USB 2.0 (Type-A)
2*USB 2.0 (Header)

	COM
	10*RS-232 (Header)

	Audio
	1*Line-out+1*MIC

	Mother Board Type
	Mini-ITX


QY-U1000
1-3.H470 Mother Board Specification:


	

	Mother Board Model
	QY-12S2A-H610-X

	Chipset
	Intel H610, Support Intel Core 12/13/14th-i3/i5/i7/i9 / Pentium / Celeron desktop CPU, LGA 1700

	Memory
	Support DDR4-3200 MHz, 2*non-ECC U-DIMM Slots, Up to 64GB

	Storage
	1*M.2 NVME SSD slot
1*SATA 3.0 SSD slot

	Display
	1*VGA: Resolution max up to 1920*1200@60Hz
1*HDMI: Resolution max up to 4096*2160@30Hz

	Expansion
	1*PCIE 16x slot
1*M.2 Key-E slot, Support WIFI module

	Ethernet
	2*Realtek RTL8111H GbE LAN Chip (10 / 100 / 1000 /2500 Mbps, RJ-45 Type)

	USB
	4*USB 3.2 (Type-A)
6*USB 2.0 (Type-A)
2*USB 2.0 (Header)

	COM
	10*RS-232 (Header)

	Audio
	1*Line-out+1*MIC

	Mother Board Type
	Mini-ITX


QY-U1000
1-4.H610 Mother Board Specification:

	

QY-U1000
2.Device Specification:

	Power Input
	1U ATX Power Module (300w / 500w / 800w / 1000w / 1300w)

	
	Support Auto-Start

	Working Temperature
	-30℃~70℃, Support 24/7 Working

	Structure
	Fully Enclosed Aluminum Alloy Material

	Heat Dissipation
	Fan Design

	Installation
	Desktop / Embedded

	Size
	485mm*250mm*44.5mm

	System
	Windows and Linux

	Mother Board Type
	Mini-ITX

	GPU
	Non-support


















	




	
QY-U1000
3.Ordering Information:

	Model
	Chipset
	CPU
	LAN
	USB
	COM
	RAM
	Display
	SSD
	Expansion

	QY-U1000
	B81
	4th
	2
	6*3.0
10*2.0
	1*RS-232/485
9*RS-232
	2*DDR 3
Up to 16GB
	1*HDMI
1*VGA
	1*MSATA
2*SATA
	1*Mini PCIE
1*PCIE 16x

	
	H110
	6th/7th/8th/9th
	
	8*3.0
8*2.0
	1*RS-232/485
9*RS-232
	2*DDR 4
Up to 32GB
	1*VGA
1*HDMI
	1*MSATA
2*SATA
	1*Mini PCIE
1*PCIE 16x

	
	H470
	10th
	
	6*3.0
6*2.0
	10*RS-232
	2*DDR 4
Up to 64GB
	1*VGA
1*HDMI
	1*M.2 SATA
1*SATA
	1*M.2
1*PCIE 16x

	
	H610
	12th/13th/14th
	
	4*3.2
8*2.0
	10*RS-232
	2*DDR 4
Up to 64GB
	1*HDMI
1*VGA
	1*M.2 PCIE
1*SATA
	1*M.2
1*PCIE 16x





4.System Information:


	CPU
	System

	4th / 6th / 7th
	Windows 7 / 10 and Linux

	8th / 9th / 10th / 12th / 13th / 14th
	Windows 10 / 11 and Linux

















5.Fittings Information:

QY-U1000

	RAM
	DDR 3
	4GB / 8GB

	
	DDR 4
	4GB / 8GB / 16GB / 32GB

	SSD
	MSATA
	64GB / 128GB / 256GB / 512GB / 1TB

	
	M.2 NVME / SATA
	128GB / 256GB / 512GB / 1TB / 2TB / 4TB

	
	SATA
	120GB / 128GB / 240GB / 256GB / 480GB / 512GB / 960GB / 1TB / 2TB / 4TB

	GSM Module
	4G
	4G+GPS

	WIFI Module
	7260AC / AX210

	ATX Power
	300w / 500w / 800w / 1000w / 1300w



6.Package List:



	Power Cable
	1*Power Cable





















7.Dimensions:

QY-U1000
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